Host And Device Specific Link Options

^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^

.. versionadded:: 3.18

When a device link step is involved, which is controlled by

:prop\_tgt:`CUDA\_SEPARABLE\_COMPILATION` and

:prop\_tgt:`CUDA\_RESOLVE\_DEVICE\_SYMBOLS` properties and policy :policy:`CMP0105`,

the raw options will be delivered to the host and device link steps (wrapped in

``-Xcompiler`` or equivalent for device link). Options wrapped with

:genex:`$<DEVICE\_LINK:...>` generator expression will be used

only for the device link step. Options wrapped with :genex:`$<HOST\_LINK:...>`

generator expression will be used only for the host link step.